Sandy Point Refinery

Biodiesel Unit Handover Report

From: Jake Thompson (Night Shift)

To: Maria Rodriguez (Day Shift)

Date: 9/18/2024

Time: 0700 hours

Key Issues:

- Clog detected in Triglyceride Tank K-901

- CSTR Reactor R-901 operating normally

- Biodiesel Separator SP-94 performance stable

Action Items:

1. Investigate and clear clog in K-901:

- Tank level reading inconsistent with feed rate

- Suspect build-up near outlet valve

- Maintenance team scheduled for 0900 hours

2. Monitor methanol feed rate from K-902

3. Check biodiesel quality (S-23) at 1000 and 1400 hours